# UDP over TCP - sing-box
The universal proxy platform.
Author: nekohasekai

Skip to content

# UDP over TCP

It's a proprietary protocol created by SagerNet, not part of shadowsocks.

The UDP over TCP protocol is used to transmit UDP packets in TCP.

### Structure

    {
      "enabled": true,
      "version": 2
    }

The structure can be replaced with a boolean value when the version is not specified.

### Fields

#### enabled

Enable the UDP over TCP protocol.

#### version

The protocol version, `1` or `2`.

2 is used by default.

### Application support

Project | UoT v1 | UoT v2
--- | --- | ---
sing-box | v0 (2022/08/11) | v1.2-beta9
Clash.Meta | v1.12.0 (2022/07/02) | v1.14.3 (2023/03/31)
Shadowrocket | v2.2.12 (2022/08/13) | /

### Protocol details

#### Protocol version 1

The client requests the magic address to the upper layer proxy protocol to indicate the request: `sp.udp-over-tcp.arpa`

#### Stream format

ATYP | address | port | length | data
--- | --- | --- | --- | ---
u8 | variable | u16be | u16be | variable

ATYP / address / port: Uses the SOCKS address format, but with different address types:

ATYP | Address type
--- | ---
`0x00` | IPv4 Address
`0x01` | IPv6 Address
`0x02` | Domain Name

#### Protocol version 2

Protocol version 2 uses a new magic address: `sp.v2.udp-over-tcp.arpa`

##### Request format

isConnect | ATYP | address | port
--- | --- | --- | ---
u8 | u8 | variable | u16be

isConnect: Set to 1 to indicates that the stream uses the connect format, 0 to disable.

ATYP / address / port: Request destination, uses the SOCKS address format.

##### Connect stream format

length | data
--- | ---
u16be | variable

##### Non-connect stream format

As the same as the stream format in protocol version 1.